<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.36.0-Maidenhead">
  <identifier>https://gis.blm.gov/arcgis/rest/services/admin_boundaries/BLM_Natl_AdminUnit/MapServer/3</identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title>BLM Administrative Unit Field Boundary</title>
  <abstract>This feature class is the Field Office level data from the feature level Dataset for the BLM Administrative Unit Boundaries Data Standard. The feature dataset includes both BLM administrative land areas and office locations. Land areas are depicted with polygons for the smallest administrative unit (field offices). Larger administrative units, such as district offices, and administrative states may be derived from these polygons. Office locations at each level are depicted with points..

This dataset is a subset of the official national dataset, containing features and attributes intended for public release and has been optimized for online map service performance. The Implementation Guide represents the official national dataset from which this dataset was derived.</abstract>
  <links>
    <link format="" size="" url="https://gis.blm.gov/arcgis/rest/services/admin_boundaries/BLM_Natl_AdminUnit/MapServer/3" type="WWW:LINK" description="" mimeType="" name="Source"/>
  </links>
  <dates/>
  <fees></fees>
  <rights>BLM Admin State</rights>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt></wkt>
      <proj4>+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs</proj4>
      <srsid>3857</srsid>
      <srid>3857</srid>
      <authid>EPSG:3857</authid>
      <description>WGS 84 / Pseudo-Mercator</description>
      <projectionacronym>merc</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial maxz="nan" miny="2978926.90280000120401382" minz="nan" dimensions="2" minx="-19942308.8960999995470047" maxx="20012451.78019999712705612" crs="EPSG:3857" maxy="10775427.45480000227689743"/>
  </extent>
</qgis>
